Hardware:

* Soldering

Firmware & Software:

* Listen to the phototransistor status and determine the state
* It travel in the right path
* Synchronized two motors so it moves in a straight line(encoder),
* Speed control- input speed and control the pwm